**Tube Opener**

**Printing stringency**: Low

**Our condition**

* Layer height: 0.1
* Infill: 20%
* Supports: No
* 210 °C, with PLA

**Features**

* Components:
  + **Tube opener**
* With three parts, to open 1.5 ml microtube cap, 0.6 ml microtube cap, and screwed cap.

v1.0: Bod Owens, 2022/07/16

****

****